LITTLE COLORADO SANITARY DISTRICT
SOLIDS SEPARATION TANK INSPECTION FORM
(Manual Write-In Form - September 2026)
	NOTICE REGARDING INSPECTION REQUIREMENTS
Under Article II, Section 2(D) of the District's Third Amended Rules and Regulations, all Solids Separation Tanks (SSTs) must be inspected every 8 years. Inspections include: (1) Measurement of scum and sludge to determine pumping need; and (2) Structural Integrity Inspection (if tank is pumped). Regardless of sludge/scum findings, a full pumping and structural inspection is required at least every 16 years.
Structures with grease traps or interceptors must have their SSTs inspected annually and must include: (1) Measurement of scum and sludge to determine pumping need; and (2) Structural Integrity Inspection (if tank is pumped). Regardless of sludge/scum findings, a full pumping and structural inspection is required at least every 4 years.
If pumping is required at an 8-year inspection, or at a 4-year inspection for structures with grease traps or interceptors, the structural inspection must be performed at the same time. Failure to comply may result in enforcement action.

	1. Property Information

	Property Address: ________________________________
________________________________________________
	Tax Parcel No.: _____________________

	2. Current Owner Information

	Owner Name: _____________________________________________

	3. Inspector Information

	Inspector: ________________________________
	License #: _______________________

	Company: ________________________________
	Phone: _________________________

	Email: __________________________________________

	4. Site and Usage Information

	Use: ☐ Residential   ☐ Commercial        # Tanks: __________________

	Grease Trap? ☐ Yes   ☐ No        Occupancy:  ☐ Full   ☐ Seasonal   ☐ Intermittent

	5. Tank Inspection & Pumping Information

	Date of last inspection: ______________________
	Date of last pumping: _______________________

	Scum Thickness (SC):
	____________________   inches

	Sludge Thickness (SL):
	____________________   inches

	Liquid Depth (DW):
	____________________   inches


If (SC + SL) / DW > 33%  →  Tank must be pumped.
	Top of scum to top of outlet baffle (SBT) - If <1 inch, pump: ____________

	Bottom of scum to bottom of outlet baffle (SBB) - If <3 inches, pump: ____________

	Was the tank pumped? ☐ Yes   ☐ No   

	If No - Reason: ☐ <33% filled   ☐ Tank not in operation   

	Other reason: ____________________________________________________________________________________
________________________________________________________________________________________________

	5. Tank Inspection & Pumping Information - Continued

	Liquid level: ☐ Normal   ☐ Low   ☐ High   ☐ Unknown   

	Depth of soil cover over access port: ________________
	Tank riser: ☐ Present   ☐ Absent

	Tank Construction: ☐ Metal   ☐ Concrete   ☐ Fiberglass    Other: __________________________

	Compartments: ☐ One   ☐ Multiple    Capacity (gallons): __________________

	Baffles - Inlet: ☐ Present   ☐ Absent        Outlet:  ☐ Present   ☐ Absent

	Clean-out on outlet side? ☐ Yes   ☐ No    Distance: __________________________

	Effluent filter present/cleaned? ☐ Yes   ☐ No   

	Reason if not cleaned: _______________________________________________________________________________
___________________________________________________________________________________________________

	Home pump station? ☐ Yes   ☐ No   

	Repairs/maintenance performed? ☐ Yes   ☐ No   

	Explain: ___________________________________________________________________________________________
___________________________________________________________________________________________________ 
___________________________________________________________________________________________________


	5A. Structural Integrity Inspection (requires pumping)

	☐ Tank shell/lid sound     ☐ Minor surface issues     ☐ Major deterioration

	☐ Access lids secure and rated for load

	☐ Inlet baffle intact     ☐ Outlet baffle intact     ☐ Baffle damage observed

	☐ Seams/joints intact     ☐ Leakage observed

	☐ No infiltration/exfiltration     ☐ Leakage present

	☐ Site free of stressors (traffic, roots, loading)     ☐ Stress observed

	Structural Summary: ☐ Sound   ☐ Minor Issues (monitor)   ☐ Significant Issues   

	If Significant Issues: ☐ Repair   ☐ Replace   

	Inspector Notes: ____________________________________________________________________________________
__________________________________________________________________________________________________
__________________________________________________________________________________________________

	6. Inspection Summary

	Is the tank functioning properly until next inspection? ☐ Yes   ☐ No   

	Recommended improvements: ________________________________________________________________________
___________________________________________________________________________________________________
___________________________________________________________________________________________________

	7. Inspector Certification


I certify this inspection was completed to the best of my knowledge.
	Inspector's Name: _____________________________
	Date: ________________________________

	Inspector's Signature: ______________________________
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NOTICE REGARDING INSPECTION REQUIREMENTS   Under Article II, Section 2(D) of the District's Third Amended Rules and Regulations, all Solids Separation Tanks (SSTs)  must be inspected every 8 years. Inspections include: (1) Measurement of scum and sludge to determine pumping need;  and (2) Structural  Integrity Inspection (if tank is pumped). Regardless of sludge/scum findings, a full pumping and structural  inspection is required at least every 16 years.   Structures with grease traps or interceptors must have their SSTs inspected annually and must include: (1) Measurement of  scum and sludge to determine pumping need; and (2) Structural Integrity Inspection (if tank is pumped). Regardless of  sludge/scum find ings, a full pumping and structural inspection is required at least every 4 years.   If pumping is required at an 8 - year inspection, or at a 4 - year inspection for structures with grease traps or interceptors, the  structural inspection must be performed at the same time. Failure to comply may result in enforcement action.  

1. Property Information  

Property Address:  ____________________ ____________   ________________________________________________  Tax Parcel No.:  _____________________  

2. Current Owner Information  

Owner Name:  _______________________ ______________________  

3. Inspector Information  

Inspector:  _______________________ _________  License #:  _______________________  

Company:  ________________________ ________  Phone:  _________________________  

Email:  _________________________ _________________  

4. Site and Usage Information  

Use:  ☐   Residential    ☐   Commercial        # Tanks: __________________  

Grease Trap?  ☐   Yes    ☐   No        Occu p ancy:   ☐   Full    ☐   Seasonal    ☐   Intermittent  

5. Tank Inspection & Pumping Information  

Date of last inspection:  ________________ ______  Date of last pumping:  __________________ _____  

Scum Thickness (SC):  ________________ ____     inches  

Sludge Thickness (SL):  ________________ ____     inches  

Liquid Depth (DW):  ________________ ____     inches  

If (SC + SL) / DW > 33%  →  Tank must be pumped.  

Top of scum to top of outlet baffle (SBT)  -   If <1 inch, pump:  ____________  

Bottom of scum to bottom of outlet baffle (SBB)  -   If <3 inches, pump:  ____________  

Was the tank pumped?  ☐   Yes    ☐   No     

If No  -   Reason:  ☐   <33% filled    ☐   Tank not in o p eration     

Other reason:  ______________________ ______________________________________________________________   ________________________________________________________________________________________________  

5. Tank Inspection & Pumping Information  -   Continued  

Liquid level:  ☐   Normal    ☐   Low    ☐   Hi g h    ☐   Unknown     

Depth of soil cover over access port:  ____________ ____  Tank riser:  ☐   Present    ☐   Absent  

